**Thông số kỹ thuật thiết bị 4G Router**

| **Hạng mục** | **Thông số kỹ thuật** |
| --- | --- |
| Hình ảnh chung |  |
| Main CPU | MT7628KN 580MHz MIPS® 24KEc™ CPU |
| Memory | Embedded with 64Mbit/8MB memory |
| FLASH | SPI 16Mbit/2MB |
| Protocol | IEEE802.11b/802.11g/802.11n/802.3/802.3u |
| Wi-Fi speed | 2.4g 2T2R 300Mbps |
| Frequency | 2.4GHZ |
| Antenna | 2\*5dB 2.4G \*2R2 external antenna |
| 2\*5bB 4G\*2R2 external antenna |
| Port | 1\*Sim card port |
| 1\*Wan |
| 2\*Lan |
| 1\*DC port |
| LED | Power, 2.4G wireless, WAN, LAN1, LAN2, 4G network |
| Button | 1\*Reset button |
| AP adaptor | DC 12V/1A |
| Max power consumption | <10W |
| Size/Color | Size:260\*227\*40 MM(Packing) |
| Color: White (Accept OEM) |
| **4G Bands** | |
| Chipset: ASR1802S | FDD-LTE： B1、B3、B5、B8 |
|  | TDD-LTE: B34、B38、B39、B40、B41 |
|  | WCDMA/UMTS:B1、B5、B8 |
|  |  |
| **Firmware specification** | |
| WAN Interface | dynamic IP, static IP, 3G (4G) dialing,PPPoE |
| Working Mode | 4G ROUTER; |
|  | AP |
| DHCP server | DHCP server |
|  | Client list |
|  | Static address allocation; |
| Support OS | SDK，ECOS |
| Virtual server | Port forwarding |
| Security | Port- (Protocol-) based filter |
|  | MAC-based filter |
| DDNS | N/A |
| VPN Tunneling | N/A |
| Bandwidth control support | Support-4G LTE |
| Static routing | Support |
| System log | Support |
| Other function | Profile import and export |
| Mac address clone |
| Web software upgrade |
| traffic statistics |
| Accessories | 1\* User manual |
|  | 1\* Power adapter (national standard 12V/1A, wire length 1.5M) |
| Packing | Neutral English packaging |
| Product net weight |  |
| Total weight |  |